**Dennis Snow A/V Requirements**

**For audiences of 250+**

LCD projector (10,000 lumens or above) and screen.

Wireless hand held or wireless lavaliere microphone.

Dedicated sound system, mixing board, and speakers (not the room’s ceiling speakers).

Minimum 24-inch high riser, at least 16 feet wide.

First row of chairs or tables no more than 10 feet from the riser or stage.

Dedicated and controllable stage lighting that provides a full stage wash. Truss lighting for larger audiences (500+) or light trees for smaller audiences.

**For Audience of less than 250:**

LCD projector (5,000 lumens or above) and screen.

Wireless hand held or wireless lavaliere microphone.

Dedicated sound system, mixing board, and speakers (not the room’s ceiling speakers).

Minimum 18-inch high riser, at least 16 feet wide.

First row of chairs or tables no more than 10 feet from the riser or stage.

To ensure proper lighting, the front of the room needs to be **BRIGHTLY** lit with either dedicated lighting (controllable light trees) or bright room lighting. If available room lighting is used, any ceiling lights directly over the projection screen must be disabled.