# ||| drum café av and staging requirements

|  |  |
| --- | --- |
| **Up to 25 participants** | No AV requirements necessary. |
| **25 to 100 participants, theatre style** | * 2 x Powered Speakers * 2 x Speaker Stands * 1 x Wireless Headset (**equiv. to DPA 4088 Core directional with microdot connector**.) **NO Lavaliere, please.** * Sufficient cabling for all connections * Sufficient amplification for all speakers   **Staging**: For events larger than 50, 16ft wide x 12 ft deep x 18 inches high riser. Please leave approximately 4 feet width of space between front of staging and first row of chairs. |
| **100 to 150 participants, theatre style** | * 2 x 15-inch full range speaker cabinets * 2 x Speaker Stands * 1 x floor monitor speaker * 8-channel mixing console with 48V phantom power * 2 x tripod boom microphone stands * 2 x Microphones equivalent to Shure SM57 or PG81 * 1 x Wireless Headset (**equiv. to DPA 4088 Core directional with microdot connector**.) **NO Lavaliere, please.** * Sufficient cabling for all connections * Sufficient amplification for all speakers   **Staging**: 16ft wide x 12ft deep x 18 inches high. Please leave approximately 4 feet width between front of staging and first row of chairs. |
| **150 to 250 participants, theatre style** | * 2 15-inch full range speaker cabinets * 2 x Speaker Stands * 1 x floor monitor speaker * 8-channel mixing console with 48V phantom power * 3 x tripod boom microphone stands * 1 x Microphone equivalent to Shure Beta 52a * 2 x Microphones equivalent to Shure SM57 or PG81 * 1 x Wireless Headset (**equiv. to DPA 4088 Core directional with microdot connector**.) **NO Lavaliere, please.** * Sufficient cabling for all connections * Sufficient amplification for all speakers * AV technician   **Staging**: 16ft wide x 16ft deep x 18 inches high. Please leave approximately 4 feet width between front of staging and first row of chairs. |
| **250 to 500 participants, theatre style**  **(OR 100-250 participants around tables)** | * 4 15-inch full range speaker cabinets * 4 x Speaker Stands * 1-2 x floor monitor speakers * 8-channel mixing console with 48V phantom power * 4 x tripod boom microphone stands * 1 x Microphones equivalent to Shure Beta 52a * 3 x Microphones equivalent to Shure SM57 or PG81 * 1 x Wireless Headset (**equiv. to DPA 4088 Core directional with microdot connector**.) **NO Lavaliere, please.** * Sufficient cabling for all connections * Sufficient amplification for all speakers   A technician **Staging**: 16ft wide x 16ft deep x 18 inches high. Please leave approximately 4 feet width between front of staging and first row of chairs. |
| **500 to 1000 participants**  **(OR 250-500 participants around tables)** | * Minimum of 4 15-inch full range speaker cabinets, preferably 6 * 4-6 x Speaker Stands * 2-3 x floor monitor speakers * Sufficient amplification for all speakers * 12-channel mixing console with 48V phantom power * 5 x tripod boom microphone stands * 2 x Microphones equivalent to Shure Beta 52a * 3 x Microphones equivalent to Shure SM57 or PG81 * 1 x Wireless Headset (**equiv. to DPA 4088 Core directional with microdot connector**.) **NO Lavaliere, please.** * Sufficient cabling for all connections * A technician * 2 large Video walls (one on either side of stage) OR 1 Video wall above the stage, optional * Camera and camera operator, optional   **Staging**: 16ft wide x 16ft deep x 18 inches high. Please leave approximately 4 feet width between front of staging and first row of chairs. |

# ||| recommended seating set up

## 1) Less than 200 participants

The room’s widest wall

12’ x 16’ (min)

# Riser